Step 1 : Run the installer
Step 2 : When installer asks for a key enter : SHOCK0-000000-123456-252525-111111-222222-333333-082735-738946-273635
Step 3 : During the end of setup installer mention the used serial is not valid, open your process monitor and kill 
	 the PRTG Server Administrator process. Setup will contiue and finish.
Step 4 : Stop both PRTG services, then copy over the three files included in the crack.zip
Step 5 : Start the PRTG services again.

Happy PRTG'ing
